(footprint "ESP32_DevKitC_RYMCU"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 2.54 -1.27 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f90805cc-4d4b-41fe-be1f-935a6ccd7187")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ESP32_DevKitC_RYMCU"
		(at 13.95 27.36 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "073466aa-48f6-40ac-959a-562ae10316f4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 13.95 26.36 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "77aad992-a83f-4438-956f-713db2195079")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 13.95 26.36 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8145992e-dad2-4c89-a3c7-32f709709fbe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start 0 0)
		(end 27.9 54.72)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "68b0d5d5-8795-47a1-ae4e-291796a3f18e")
	)
	(fp_rect
		(start 0 6.52)
		(end 27.9 54.72)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "410419f6-9a84-431d-b0fe-ea63c5dab233")
	)
	(fp_text user "${REFERENCE}"
		(at 13.95 28.86 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b28476b5-8745-46f2-84ff-ed88578518c6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 1.27 7.62)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4d908c32-ee53-4cd8-8dd8-c83526125db9")
	)
	(pad "2" thru_hole circle
		(at 1.27 10.16)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ecdf825f-df08-4035-8d59-cb6ed4c24beb")
	)
	(pad "3" thru_hole circle
		(at 1.27 12.7)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "09cd60d4-d6d7-4cf1-a67c-610276979a7e")
	)
	(pad "4" thru_hole circle
		(at 1.27 15.24)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "12d78e63-c037-4eec-b366-5d94448f5d25")
	)
	(pad "5" thru_hole circle
		(at 1.27 17.78)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "06d3a89d-fe67-4daa-84f2-6bd31d59e5ef")
	)
	(pad "6" thru_hole circle
		(at 1.27 20.32)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d4a098e4-c1e5-43aa-8e75-4228d19e6511")
	)
	(pad "7" thru_hole circle
		(at 1.27 22.86)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "16512920-dc5f-4c6c-9b0c-27510285db55")
	)
	(pad "8" thru_hole circle
		(at 1.27 25.4)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "45aac27f-9f05-4f81-ad09-0714c25504c8")
	)
	(pad "9" thru_hole circle
		(at 1.27 27.94)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7a997b1c-f21f-46d3-9347-959ee7d9f1de")
	)
	(pad "10" thru_hole circle
		(at 1.27 30.48)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "57e29aee-4c51-4516-bbfa-a8bd80a4c00c")
	)
	(pad "11" thru_hole circle
		(at 1.27 33.02)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ea89ec96-b8c5-4335-bb7e-597c316eff94")
	)
	(pad "12" thru_hole circle
		(at 1.27 35.56)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fd2e9e48-33f4-497d-9ffb-12eed7bccfe2")
	)
	(pad "13" thru_hole circle
		(at 1.27 38.1)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4670b0d7-cb62-4979-89e0-e63d08cfd26d")
	)
	(pad "14" thru_hole circle
		(at 1.27 40.64)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "227f099d-a257-42c4-bd36-cd213080e3c2")
	)
	(pad "15" thru_hole circle
		(at 1.27 43.18)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a3850576-c175-4b64-94dd-d75b5cb187f9")
	)
	(pad "16" thru_hole circle
		(at 1.27 45.72)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ee7ad67b-e7ae-4d9f-beb8-a352c3eaf871")
	)
	(pad "17" thru_hole circle
		(at 1.27 48.26)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c35dae6-968e-49f8-b904-1fac85e3393a")
	)
	(pad "18" thru_hole circle
		(at 1.27 50.8)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0cfb47e4-44a9-4816-b89a-579900cee929")
	)
	(pad "19" thru_hole circle
		(at 1.27 53.34)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8916e867-5855-460d-a74f-a27707253b96")
	)
	(pad "20" thru_hole circle
		(at 26.67 7.62)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "129091dd-4697-48d5-b76e-dd59a66c0ad5")
	)
	(pad "21" thru_hole circle
		(at 26.67 10.16)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "919d2459-ee68-45a1-9d9d-ba99370a6dc2")
	)
	(pad "22" thru_hole circle
		(at 26.67 12.7)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "24e6209d-35c1-42c3-af63-bf831ee21d7e")
	)
	(pad "23" thru_hole circle
		(at 26.67 15.24)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b2d91fe8-e1de-4bfe-bbee-aa3bef091b6d")
	)
	(pad "24" thru_hole circle
		(at 26.67 17.78)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "734323f3-75ac-46f9-9079-1211d7454270")
	)
	(pad "25" thru_hole circle
		(at 26.67 20.32)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "18cac653-2b82-47ec-aa9f-69d70415c651")
	)
	(pad "26" thru_hole circle
		(at 26.67 22.86)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "09fc6e3e-9085-4ca5-8e2f-11df51d2fcd5")
	)
	(pad "27" thru_hole circle
		(at 26.67 25.4)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2dbeceec-2c22-458c-9750-f8127d7421ea")
	)
	(pad "28" thru_hole circle
		(at 26.67 27.94)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b9dc4bd4-b2c1-4a09-b6bc-d9d7c8f2afd6")
	)
	(pad "29" thru_hole circle
		(at 26.67 30.48)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d0e31f52-bb07-4ee5-8282-653990482522")
	)
	(pad "30" thru_hole circle
		(at 26.67 33.02)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5b9d293c-3fd1-454c-9819-d9a844c69a07")
	)
	(pad "31" thru_hole circle
		(at 26.67 35.56)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bab5e48e-f53b-4398-a169-4ed56a7bb1ec")
	)
	(pad "32" thru_hole circle
		(at 26.67 38.1)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e94dc7d1-3da4-4b89-bbad-fae698e32613")
	)
	(pad "33" thru_hole circle
		(at 26.67 40.64)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "71dd4fab-106d-460f-8d64-b2c8b23ef31b")
	)
	(pad "34" thru_hole circle
		(at 26.67 43.18)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a2aeac4c-6dbc-4893-baaf-38dd95940827")
	)
	(pad "35" thru_hole circle
		(at 26.67 45.72)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8aba11e9-b351-494b-a249-87bf14dce163")
	)
	(pad "36" thru_hole circle
		(at 26.67 48.26)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d2497308-c801-4a35-b253-bd28976a86db")
	)
	(pad "37" thru_hole circle
		(at 26.67 50.8)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8d2f081f-d314-4943-b49a-465d242bc0e2")
	)
	(pad "38" thru_hole circle
		(at 26.67 53.34)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a8230a12-5c94-4632-a656-9c3fe10f121a")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(uuid "09d3fc69-13c2-4142-9898-59b96eeaa21d")
		(name "No routing")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 0) (xy 27.9 0) (xy 27.9 6.52) (xy 0 6.52)
			)
		)
	)
	(embedded_fonts no)
)
