(footprint "Transformer_220_5_1A_Module"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -12.6 -11.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "caaf2c29-9fab-4ebe-8fc8-4544a0b601eb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15875)
			)
		)
	)
	(property "Value" "Transformer_220/5_1A_Module"
		(at 0 11 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e8002a30-de96-403d-a118-43e8fb0ccd3f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "82149ce1-b99a-44fb-96ec-2ab80849a45d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "76cd516d-fc85-4d42-bd0d-7c038e87d23b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -14.95 6.77)
		(end -13.62 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a9ad7a2a-425e-4915-81db-ae21254d6710")
	)
	(fp_line
		(start -14.95 8.1)
		(end -14.95 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0cdadd8a-ab8e-41d8-a5e6-cb687d29274f")
	)
	(fp_line
		(start -12.35 6.77)
		(end -7.21 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "398a06cb-de44-45a1-ae15-4b68df40a61a")
	)
	(fp_line
		(start -12.35 9.43)
		(end -12.35 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ddfc0ab8-0f67-4bb8-b2cd-39199141aef7")
	)
	(fp_line
		(start -12.35 9.43)
		(end -7.21 9.43)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "26128a49-7993-4a56-ad7d-4af3f4066bbc")
	)
	(fp_line
		(start -7.21 9.43)
		(end -7.21 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dbf47577-be91-40b8-9dee-93017f253d85")
	)
	(fp_line
		(start 9.73 6.77)
		(end 11.06 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "05b30b40-f9fc-4617-b382-c5c44bc07232")
	)
	(fp_line
		(start 9.73 8.1)
		(end 9.73 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "eb1e018a-9555-47ef-bc7e-5b1034bda958")
	)
	(fp_line
		(start 12.33 6.77)
		(end 14.93 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0ac30cc0-7458-4698-a3c3-7771bc02304c")
	)
	(fp_line
		(start 12.33 9.43)
		(end 12.33 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1ae1ee4c-c4eb-4ed8-8a8b-47a7c1dd8443")
	)
	(fp_line
		(start 12.33 9.43)
		(end 14.93 9.43)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b9457030-bbcd-41a5-9b6c-e749434778cc")
	)
	(fp_line
		(start 14.93 9.43)
		(end 14.93 6.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0a6a2e53-4b80-4fe0-a63e-10540e1700df")
	)
	(fp_rect
		(start -15 -10.5)
		(end 15 9.5)
		(stroke
			(width 0.254)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "da790940-a745-4ac2-a959-dbf0f8233eed")
	)
	(fp_line
		(start -14.89 7.465)
		(end -14.255 6.83)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8f8ffc37-bf7c-4271-9d52-7e7a7487b4ad")
	)
	(fp_line
		(start -14.89 9.37)
		(end -14.89 7.465)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6a284d45-7a96-407f-838e-115c605cc3d5")
	)
	(fp_line
		(start -14.255 6.83)
		(end -7.27 6.83)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a34505a5-b8fb-4efe-8581-861e55951131")
	)
	(fp_line
		(start -7.27 6.83)
		(end -7.27 9.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "048898e9-55de-4a34-8b0f-8ea0980abf46")
	)
	(fp_line
		(start -7.27 9.37)
		(end -14.89 9.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3adffad4-814c-4868-bcb1-a6cfa41ed646")
	)
	(fp_line
		(start 9.79 7.465)
		(end 10.425 6.83)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cc5aabd3-3bcf-4ab7-9ec1-15d25e14bedf")
	)
	(fp_line
		(start 9.79 9.37)
		(end 9.79 7.465)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7c9e8e68-62af-4f93-be66-03b3174b616a")
	)
	(fp_line
		(start 10.425 6.83)
		(end 14.87 6.83)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "07778d00-3a2d-4025-a484-7b8646d8ac7c")
	)
	(fp_line
		(start 14.87 6.83)
		(end 14.87 9.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "64c49d72-1df8-4120-8b64-c65f8aa2f8c1")
	)
	(fp_line
		(start 14.87 9.37)
		(end 9.79 9.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fc9506a7-7049-4ced-8afb-9f6abf07fee6")
	)
	(fp_text user "V-"
		(at 11 5 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "7a811511-54ef-42fe-aac4-04b55e02da43")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15875)
			)
		)
	)
	(fp_text user "N"
		(at -8.509 5.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "849e0305-c0cd-4e84-92ac-8f9c5303cd13")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15875)
			)
		)
	)
	(fp_text user "V+"
		(at 13.6 5 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a6ee0f8f-072b-416b-87f6-94af7f46cdfd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15875)
			)
		)
	)
	(fp_text user "L"
		(at -13.6 5.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c4ab9a46-aa6e-4ce4-a01f-300571d779c1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15875)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 12.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7cba04c1-ad08-43c1-99fe-100f9706e3ff")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -13.62 8.1 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2bf4194c-11d7-4a14-8ca2-264838ad4377")
	)
	(pad "2" thru_hole oval
		(at -8.54 8.1 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8ebf881d-9c13-462c-80bc-cd4927c19cfc")
	)
	(pad "3" thru_hole oval
		(at 13.6 8.1 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "54e638f0-c8e1-4208-936d-a05ad24e571e")
	)
	(pad "4" thru_hole rect
		(at 11.06 8.1 90)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f626e4d4-746d-4737-b656-17ede08c9408")
	)
	(embedded_fonts no)
)
