(footprint "ATK-MW8266D"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -7.5 -15.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "66aa11d5-8592-4413-b775-d71d584519b9")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ATK-MW8266D"
		(at 0 16.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5815b450-1250-4e76-9986-3ff62a23b5e8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "http://www.openedv.com/docs/modules/iot/atk-esp.html"
		(at 0 19.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0fb6cb36-8ca6-487d-8c0d-a111335a7659")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Alientek ESP8266 WiFi-uart module"
		(at 0 15.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a47c0fec-7785-421c-aac7-7e389cab5ec0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -7.68 11.85)
		(end -7.68 14.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "29d9255d-b015-4ad2-aab1-ffb5dabb1953")
	)
	(fp_line
		(start 5.08 11.85)
		(end -7.68 11.85)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f257bc4a-4fe5-4492-b32f-388fdf1eed6a")
	)
	(fp_line
		(start 5.08 11.85)
		(end 5.08 14.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8d52cd63-d2a0-491c-a22a-a0bd0865a432")
	)
	(fp_line
		(start 5.08 14.51)
		(end -7.68 14.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d943dfc9-983f-4ade-8939-62f08de85bee")
	)
	(fp_line
		(start 7.68 13.18)
		(end 7.68 14.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5d19fb20-66bc-4484-b4d6-918e676e283e")
	)
	(fp_line
		(start 7.68 14.51)
		(end 6.35 14.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ff4f5a89-b3ca-4c6d-b958-0b0f32714ce7")
	)
	(fp_rect
		(start -9.5 -14.5)
		(end 9.5 14.5)
		(stroke
			(width 0.254)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "ede2f971-8bca-4848-a9d1-5c33c5a0958a")
	)
	(fp_rect
		(start -9.5 -14.5)
		(end 9.5 14.5)
		(stroke
			(width 0.254)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "66ae0904-3f9c-4dfe-a4b7-6849aa993956")
	)
	(fp_line
		(start -7.62 11.91)
		(end 7.62 11.91)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e28763b7-19c6-4e1f-9ceb-66fdf852892f")
	)
	(fp_line
		(start -7.62 14.45)
		(end -7.62 11.91)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "eabaf0a7-21f0-4c24-9bfd-ed96f8115773")
	)
	(fp_line
		(start 6.985 14.45)
		(end -7.62 14.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9a66edeb-1224-4244-a1d9-d81e0cceb48a")
	)
	(fp_line
		(start 7.62 11.91)
		(end 7.62 13.815)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e6e525c7-36c9-4a03-95d4-95538bda6255")
	)
	(fp_line
		(start 7.62 13.815)
		(end 6.985 14.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c8951726-0351-4973-93ca-d06384388a9f")
	)
	(fp_text user "ATK ESP8266"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e0dd6b14-8a07-41e1-bf80-301e6b2dcdf6")
		(effects
			(font
				(size 1 1)
				(thickness 0.125)
			)
		)
	)
	(fp_text user "Antenna"
		(at 0 -8 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "0f6ce970-b525-479d-ad3d-f11982c77192")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.1)
			)
		)
	)
	(fp_text user "KEEP-OUT ZONE"
		(at 0 -10.5 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "c0ab660f-d948-4406-911e-3c72f96f67c4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 18 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b75931b7-2a21-4ae4-b19c-43cca2d6041c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 6.35 13.18 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "18e8dd2e-b72c-4db4-932f-c11db201eebf")
	)
	(pad "2" thru_hole oval
		(at 3.81 13.18 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6d442aff-a326-47ff-9bc9-8c42d38b71eb")
	)
	(pad "3" thru_hole oval
		(at 1.27 13.18 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "82e78d8f-8e07-4ce4-9659-582bda8e9df7")
	)
	(pad "4" thru_hole oval
		(at -1.27 13.18 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cb113e47-fafd-4bf0-ba84-662108a9f031")
	)
	(pad "5" thru_hole oval
		(at -3.81 13.18 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f411c3ad-52b0-4635-85e6-8add0231b772")
	)
	(pad "6" thru_hole oval
		(at -6.35 13.18 270)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b6e7b4aa-4a6f-4fcb-9d38-766ecbc7e6d7")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(uuid "d80086d3-2edd-4077-a281-5f9dde62f7bf")
		(name "No routing")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -9 -14) (xy -9 -5) (xy 9 -5) (xy 9 -14)
			)
		)
	)
	(group ""
		(uuid "9f51b370-845a-4d90-8d44-1d4e55cb4015")
		(members "18e8dd2e-b72c-4db4-932f-c11db201eebf" "29d9255d-b015-4ad2-aab1-ffb5dabb1953"
			"5d19fb20-66bc-4484-b4d6-918e676e283e" "6d442aff-a326-47ff-9bc9-8c42d38b71eb"
			"82e78d8f-8e07-4ce4-9659-582bda8e9df7" "8d52cd63-d2a0-491c-a22a-a0bd0865a432"
			"9a66edeb-1224-4244-a1d9-d81e0cceb48a" "b6e7b4aa-4a6f-4fcb-9d38-766ecbc7e6d7"
			"c8951726-0351-4973-93ca-d06384388a9f" "cb113e47-fafd-4bf0-ba84-662108a9f031"
			"d943dfc9-983f-4ade-8939-62f08de85bee" "e28763b7-19c6-4e1f-9ceb-66fdf852892f"
			"e6e525c7-36c9-4a03-95d4-95538bda6255" "eabaf0a7-21f0-4c24-9bfd-ed96f8115773"
			"f257bc4a-4fe5-4492-b32f-388fdf1eed6a" "f411c3ad-52b0-4635-85e6-8add0231b772"
			"ff4f5a89-b3ca-4c6d-b958-0b0f32714ce7"
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
		(offset
			(xyz 6.36 -13.2 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 90)
		)
	)
)
