(footprint "Relay_JQC-3FF-005-1Z"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hongfa subminature high power latching SPDT relay 5, 6, 9, 12, 18, 24, 48VDC. 10A switching current, Form-B https://www.generationrobots.com/media/JQC-3FF-v1.pdf")
	(tags "relays Hongmei 1-coil")
	(property "Reference" "REF**"
		(at -2 -3 0)
		(layer "F.SilkS")
		(uuid "fd0f43dc-deff-461c-bd31-27a3beb9413e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Relay_JQC-3FF-005-1Z"
		(at 7 -5 0)
		(layer "F.Fab")
		(uuid "d7e8705c-9d76-44dd-8194-796951704bf6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 7 15.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aab30ce8-a74c-41bf-8f45-7d4e93216534")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 12 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dec044f5-0ced-40cf-b2ed-80bb1a7a2ac8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -4 12.1)
		(end -4 14.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "99171971-3c81-4a22-8c9c-48d77f0c8a8d")
	)
	(fp_line
		(start -4 14.3)
		(end -1.8 14.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "131830d3-6fe5-4319-9e20-b691e40805d5")
	)
	(fp_line
		(start -3.6 -1.9)
		(end -3.6 13.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "838f0a8f-7324-4280-a908-878a6a98823c")
	)
	(fp_line
		(start -3.6 13.9)
		(end 15.8 13.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "33ba6bb8-42b1-48d9-9243-e6a0b90f186c")
	)
	(fp_line
		(start -0.4 6)
		(end 2.4 6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "474a76b7-47e3-4bec-be4e-cbebec304983")
	)
	(fp_line
		(start 2.9 3.95)
		(end 2.9 7.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d2897046-4386-4b1b-a073-011aa31676c8")
	)
	(fp_line
		(start 2.9 7.75)
		(end 4.9 7.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "82f1f9ae-930a-4ff9-9ac3-be26bb7a82ab")
	)
	(fp_line
		(start 3.9 0)
		(end 1.4 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d8ce081b-29d4-4d4b-998e-c8f7afb2d808")
	)
	(fp_line
		(start 3.9 3.95)
		(end 3.9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3bd94a4b-7a31-42fc-942b-d9505c30b9d6")
	)
	(fp_line
		(start 3.9 7.75)
		(end 3.9 12)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "28a818ea-c007-423f-914f-d6a09612d188")
	)
	(fp_line
		(start 3.9 12)
		(end 1.4 12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4a09816a-4fb2-4528-b623-29029859f318")
	)
	(fp_line
		(start 4.9 3.95)
		(end 2.9 3.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "df645c7c-d2ae-4cd0-8cf3-fef8cfad0162")
	)
	(fp_line
		(start 4.9 5.55)
		(end 2.9 6.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "67b18a82-53b1-4474-b6fb-34be6eee9015")
	)
	(fp_line
		(start 4.9 7.75)
		(end 4.9 3.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "378dc484-e631-4ddf-938d-ff1a87e5de4d")
	)
	(fp_line
		(start 6.4 6)
		(end 5.3 6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e7ef2ce8-8d9f-4a16-b154-cf68ce65a91d")
	)
	(fp_line
		(start 6.4 6)
		(end 8.2 4.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "43dab8e3-dfa6-48de-84fd-2ee408ba2eff")
	)
	(fp_line
		(start 8 2.8)
		(end 8 4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f4eb66b6-8353-481e-95ae-ecfca6372f23")
	)
	(fp_line
		(start 8 2.8)
		(end 12.2 2.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0597be12-47d4-46ae-bcf7-0440b41a86a4")
	)
	(fp_line
		(start 8 9.2)
		(end 8 8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "abf38c4f-669e-40a0-b930-a731d8c37b33")
	)
	(fp_line
		(start 12.2 1.6)
		(end 12.2 2.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "24276916-5336-43e6-a7db-94230dc5909b")
	)
	(fp_line
		(start 12.2 9.2)
		(end 8 9.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "07ccb6f5-ab53-4d0e-8414-7bbc521a2b1b")
	)
	(fp_line
		(start 12.2 10.4)
		(end 12.2 9.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4aadd050-76f0-4b35-a902-75be48d645b6")
	)
	(fp_line
		(start 15.8 -1.9)
		(end -3.6 -1.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "939d5683-2a43-4e05-8e01-ae7ac09576a4")
	)
	(fp_line
		(start 15.8 13.9)
		(end 15.8 -1.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bc5f1f15-fa5d-4a4f-a05c-67fe3aef8a12")
	)
	(fp_line
		(start -3.8 -2.1)
		(end -3.8 14.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f8f73ccd-07e6-4407-941e-f386d4134e00")
	)
	(fp_line
		(start -3.8 14.1)
		(end 16 14.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "87e640b1-c99c-41fa-b7b0-8ebd0d6ef2c8")
	)
	(fp_line
		(start 16 -2.1)
		(end -3.8 -2.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "775bf8b8-bac0-42d6-9b9f-ab6b36180b4d")
	)
	(fp_line
		(start 16 14.1)
		(end 16 -2.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7b717307-0883-4ef7-9d76-e0cc361cf439")
	)
	(fp_line
		(start -3.4 -1.7)
		(end -3.4 12.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4bacdf74-fc4f-48ab-a7ca-0e65c4803bfe")
	)
	(fp_line
		(start -3.4 12.7)
		(end -2.4 13.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f06c9a94-b8cc-49fc-ae73-3cc3b533bacf")
	)
	(fp_line
		(start -2.4 13.7)
		(end 15.6 13.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0009184d-aa19-4312-953e-b182713505da")
	)
	(fp_line
		(start 15.6 -1.7)
		(end -3.4 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "38e34458-de7d-421f-a0c5-a3f045379dc2")
	)
	(fp_line
		(start 15.6 13.7)
		(end 15.6 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "85c7b886-f11a-4157-aaad-c93ebe925452")
	)
	(fp_text user "${REFERENCE}"
		(at 6.2 6 0)
		(layer "F.Fab")
		(uuid "af70861d-430d-475b-86c5-b944e80520a7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "11" thru_hole circle
		(at -2 6)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "33d00e72-2fd6-47c4-baa1-38067895fe89")
	)
	(pad "12" thru_hole circle
		(at 12.2 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d832323f-a6d3-460a-abbc-3df3880e92e2")
	)
	(pad "14" thru_hole circle
		(at 12.2 12)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e5f366d2-b01f-461d-ba35-ae4ccaa55bc8")
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1)
		(uuid "36a20b37-5997-41a5-a8b2-8ca4b6199d3a")
	)
	(pad "A2" thru_hole circle
		(at 0 12)
		(size 2.5 2.5)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "774f9c67-df5c-4f55-b385-72e4ef19a931")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Hongfa_JQC-3FF_0XX-1Z.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${USER_3DMODEL}/JQC-3FF-005-1Z.step"
		(offset
			(xyz 5.12 -6 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
