(footprint "MEGA2560 Pro Mini"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "MEGA2560 Pro Mini"
		(at 0 -18.9484 0)
		(layer "F.SilkS")
		(uuid "50a0d442-c380-49e6-b0b7-17531583e474")
		(effects
			(font
				(size 0.9144 0.9144)
				(thickness 0.1524)
			)
			(justify left top)
		)
	)
	(property "Value" "MEGA2560 Pro Mini"
		(at -1.374 -20.7264 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "16543a2d-e0a7-414f-9331-de5030124430")
		(effects
			(font
				(size 0.9144 0.9144)
				(thickness 0.1524)
			)
			(justify left top)
		)
	)
	(property "Datasheet" ""
		(at 6.5 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d58e1746-ed84-4e57-a32b-596afea624a7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 6.5 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "bf954475-f69f-4f93-8850-3250c25833f5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -28.298 -17.6784)
		(end -28.298 -8.6868)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "20ec362d-9a69-46bd-b410-c7e9dd87d238")
	)
	(fp_line
		(start -28.298 -8.6868)
		(end -26.7994 -8.6868)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9260105e-8c3a-4505-834c-6a2dd92ba4e7")
	)
	(fp_line
		(start -28.298 -8.128)
		(end -28.298 0)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1a519da4-d047-4f3a-84b0-63c236cc7001")
	)
	(fp_line
		(start -28.298 0)
		(end -21.44 0)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "98c7b459-a88c-4a3e-ad71-3f0d3fac740e")
	)
	(fp_line
		(start -28.298 0.5842)
		(end -28.298 20.32)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "36e07802-8da1-4eec-9df9-b00570aab7df")
	)
	(fp_line
		(start -28.298 20.32)
		(end 25.7024 20.32)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d53d1b8a-768d-4745-b671-18f2ef6c48b5")
	)
	(fp_line
		(start -26.7994 -8.6868)
		(end -26.7994 0.5842)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "7a02119c-eff0-4907-99e9-985943ec4d4c")
	)
	(fp_line
		(start -26.7994 0.5842)
		(end -28.298 0.5842)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1b60f5eb-dc56-4d5d-a3df-cf37ceb9e194")
	)
	(fp_line
		(start -21.44 -8.128)
		(end -28.298 -8.128)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e83ff0ee-67a3-4815-831c-71058214c9cd")
	)
	(fp_line
		(start -21.44 0)
		(end -21.44 -8.128)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a8138bb2-3da2-4491-8e65-b59fcb309bb0")
	)
	(fp_line
		(start -9.0194 9.4488)
		(end -8.8924 9.4488)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "37f749fb-46d6-436c-b5e6-bf64c2d1faae")
	)
	(fp_line
		(start 20.851 0.508)
		(end 21.232 0.127)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "57f6cc76-a0ac-4026-bdb6-9df10544bc08")
	)
	(fp_line
		(start 20.978 0.508)
		(end 20.851 0.508)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9b2a4428-b856-470c-bd00-c459ac32c55e")
	)
	(fp_line
		(start 21.105 0.508)
		(end 20.978 0.508)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b548e24e-bb2e-451d-852a-b05472048265")
	)
	(fp_line
		(start 21.232 0.127)
		(end 21.232 0.508)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fde8df6a-9e2c-45bf-991e-0fbcabd1914c")
	)
	(fp_line
		(start 21.232 0.508)
		(end 20.978 0.508)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f5e1e78a-c1c5-4a13-94df-40149adb78d5")
	)
	(fp_line
		(start 25.7024 -17.6784)
		(end -28.298 -17.6784)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b19cdbf1-ea4f-4ecf-9dc1-b84934565e92")
	)
	(fp_line
		(start 25.7024 20.32)
		(end 25.7024 -17.6784)
		(stroke
			(width 0.127)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6757b0fc-4020-4468-ac00-54a1614d6012")
	)
	(fp_text user "A7"
		(at -6.6105 -13.29922 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "00682389-1295-43a1-929b-f9215e9b6a74")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D47"
		(at 23.4624 -13.29922 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "03b9f2e8-2f2a-47ff-af1a-3cccdccf557a")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "RESET"
		(at 19.86248 7.5928 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "03cda773-3a19-446c-818f-bb87d0056cf4")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D2"
		(at -11.8139 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0b52e091-5506-4b8b-a9c8-4b20cb0675b6")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D26"
		(at 18.42 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0e0ea49d-21d2-44aa-bea2-45a2246fff7e")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D17"
		(at 5.6519 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0e4a374c-c476-4660-9705-406e4284db0f")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D27"
		(at 18.4012 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "11600289-b3b4-4d7b-8be6-9f1b5494b8d0")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A8"
		(at -4.0898 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "11a45f05-25b6-41e1-94c3-9476342d18a4")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "VIN"
		(at -27.283 14.72618 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "122838b0-fd24-4440-a961-c65f0a3320e5")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D12"
		(at 0.6486 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "13bb45ea-bca6-4c1d-b710-75f1eb0f931a")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D35"
		(at 8.1253 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "16147aae-d379-4eb2-a709-3210d908fe43")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "AREF"
		(at -17.3628 14.72618 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "17377666-ab88-4860-8237-2aeec427c901")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D49"
		(at 21.20452 -12.1343 270)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "176b3889-d3a6-4a99-aedf-689d3be79fc7")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D53"
		(at 21.20452 -7.2118 270)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "193973e4-8a9d-441d-823a-27ce48fe8168")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "USB"
		(at -24.996 -2.413 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1f09a1db-a8a2-4168-8f66-75d6edecbbaa")
		(effects
			(font
				(size 1.016 1.016)
				(thickness 0.1016)
			)
			(justify left top)
		)
	)
	(fp_text user "D16"
		(at 5.7418 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1f91f3b8-d12c-4adb-9999-4c97e9e57d8a")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "Mega 2560 PRO (Embed)"
		(at -27.5 10.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "22abce6a-a454-4033-9d10-0db2136ab355")
		(effects
			(font
				(size 0.95992 0.95992)
				(thickness 0.1321)
			)
			(justify left top)
		)
	)
	(fp_text user "D39"
		(at 13.2026 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "268c223d-0549-44fa-96bf-18fd865f1fab")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "GND"
		(at 22.40248 7.2118 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "2ca699d7-5099-48fb-a3f2-5cf6b8258369")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D25"
		(at 15.8629 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "2e5d73ee-ffaa-4e08-afd0-63541fc1afd6")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A1"
		(at -14.3328 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3031b6fc-11d5-4ca5-9eca-6fbf85dfda98")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D48"
		(at 23.72452 -12.1343 270)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "30d7a5c6-0b6f-42ac-9a28-aa4ea13c709d")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A3"
		(at -11.7392 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "322c0498-d864-4fdb-bb43-a3b577d1716a")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D19"
		(at 8.2841 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "364ce792-3c7b-4590-8ef1-d252fd40dbf3")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D22"
		(at 13.3001 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3a547497-f0f2-4e68-a9be-a63deb5e0331")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D15"
		(at 3.089 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3a97cd31-e64c-42d5-9531-e42fcb0f33d0")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A11"
		(at -2.0611 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3ad72823-f173-4ac5-950c-e358de8f61bc")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D18"
		(at 8.1774 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3b98f2d5-c304-464d-b337-5c59707eba84")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D29"
		(at 20.9254 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4212fd2c-64c2-4180-a684-43a3097109d7")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D20"
		(at 10.7649 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "425419e3-5382-456d-a161-ed7a99daad85")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D37"
		(at 10.7532 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4493f48b-448b-4db4-b3e8-6f3d63b7d64e")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "5V"
		(at -21.8568 14.72618 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4542e97b-1220-4fb1-8fd5-53f272e1843c")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "GND"
		(at -24.7588 17.36978 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "473c9814-97c8-42b2-a8b0-7311efe4f4f9")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D50"
		(at 23.72452 -9.5623 270)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4787ef5f-c031-4839-91b9-432c1de19caf")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D13"
		(at 0.5666 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4f3c381a-ba41-4a32-88ff-d5f0d459ac59")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D7"
		(at -6.7189 17.35658 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4fe9560d-2e91-4721-b580-fafa2eaf1d46")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "TX"
		(at -14.2429 17.35658 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "504b3799-f267-47f5-b800-63413800685b")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "3V3"
		(at -19.6831 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "551fb9fa-861d-453b-ab3c-10ef4fd33c28")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D43"
		(at 18.3682 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "55c9599f-4e8e-4e4a-91be-36b841aa6cd3")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "MISO"
		(at 19.86248 2.2588 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "59199655-cfff-4319-9207-f1446cc1bbd9")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D34"
		(at 8.1236 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5c848a34-b90c-4139-9950-508cef21ce93")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D10"
		(at -1.9353 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5cd0ba60-cbda-46a0-bfd3-74e3c4b064d1")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D42"
		(at 18.3897 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5d2eef04-11c4-44ed-9f3c-894f78758856")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D5"
		(at -9.2541 17.35658 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "634b412b-0f1b-49f3-aead-0ace8b1e81c4")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "5V"
		(at 22.40248 1.7508 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "662f6d5f-b3d7-4dc7-b7b8-d9065569532b")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "SCK"
		(at 19.86248 4.5448 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "665ff8f1-64eb-4c07-a6f5-a1541a83abe3")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D38"
		(at 13.2676 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "68dc16a7-8e12-4ef6-b2ec-f967f05e8609")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D9"
		(at -4.1967 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "730158e0-9bd3-464b-af7a-402a4dc17e6c")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D6"
		(at -6.6481 14.85668 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "743c010e-5424-42a2-a9fc-482efc27fb65")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D21"
		(at 10.7482 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "74a6c5a1-3858-4769-a763-d741aab56537")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D28"
		(at 20.9323 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "76364948-b7d0-4640-97f8-33ea38c9e44d")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D30"
		(at 23.5586 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "774934e5-70b2-428b-a0b9-a794912ad47c")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A14"
		(at 3.2036 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8142c363-aea7-437b-b6dc-971ee8a2f913")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D14"
		(at 3.1739 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8184efa1-f4c3-42c2-bdd3-cbfdb775fe26")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "MOSI"
		(at 22.40248 4.9258 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "827bf841-48f0-4da2-a7e4-d5325a809d78")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D4"
		(at -9.3267 14.85318 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "85240e64-3f3d-4e79-9ead-f881fceca491")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A6"
		(at -6.6829 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8769d260-d2d9-4263-b16f-661fb03328b1")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D51"
		(at 21.20452 -9.557 270)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8a707d15-323b-413b-a85d-719baf050c54")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D24"
		(at 15.9104 14.72968 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8b88a2be-d84a-4ebc-884a-6c2d81df12ea")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D31"
		(at 23.5063 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "92c3e6cb-ffb9-421e-8142-6dd0e7239754")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D41"
		(at 15.7763 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "94828f9c-38e8-4d05-8943-aacfe5e845d8")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A9"
		(at -4.087 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "94c63901-b839-410b-a935-50025d2014bb")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D45"
		(at 20.9275 -13.29922 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "95d76f26-60eb-416f-a1ae-6af7e6ff81ea")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D46"
		(at 23.4245 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "978a8046-e7d7-4872-a58e-113b2340e412")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A2"
		(at -11.722 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "98e176c2-e8c5-46af-b208-22fbd92f175e")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D23"
		(at 13.3219 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "99ea6b47-4050-4aa6-842b-0c1542910ac0")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A4"
		(at -9.2028 -15.90062 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9b23335f-0d53-43f9-8dea-880724ecd9ac")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D52"
		(at 23.72452 -7.2118 270)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9fa0ccb2-fe4c-43e6-8493-031f6c3078cc")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D32"
		(at 5.5892 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a6723cff-419f-48d5-b644-7aac57ac515b")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "ICSP"
		(at 18.08406 5.4244 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a833060b-0bb6-41dd-ae08-14946386a0ab")
		(effects
			(font
				(size 0.90664 0.90664)
				(thickness 0.1247)
			)
			(justify left top)
		)
	)
	(fp_text user "A5"
		(at -9.2058 -13.29922 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a84ef5fb-6da7-48f2-b608-ab359ca36e23")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "RST"
		(at -17.0621 17.36978 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a87205fb-b575-4fad-821e-2ea14458c021")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D3"
		(at -11.7662 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "af18ee09-3487-4816-aa34-1eacf31ebdbb")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A15"
		(at 3.0779 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "af6420c5-9e52-48aa-94d8-684b22f20f61")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D33"
		(at 5.5495 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b9bd10b6-4fe3-4101-b236-cfaef8f8341b")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "3V3"
		(at -19.6557 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "bacee4a4-19c4-481a-9a53-e892707d07f5")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "VIN"
		(at -27.2838 17.35658 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "bfcc3493-b911-48eb-b03c-f62c259a1c24")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A12"
		(at 0.6895 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c19cc743-01be-4942-9f00-5e335dbae7dd")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "5V"
		(at -21.9066 17.35658 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "cce561ff-9341-400b-919a-830579c799b2")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D36"
		(at 10.7649 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "d2c3f1ab-9739-4bdd-aebc-d89d2a993152")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D11"
		(at -1.9488 17.35988 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "da65f76f-ba44-4a8a-9254-300a2c53047f")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "RX"
		(at -14.2797 14.72618 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "dc1a64f2-2590-45fd-a3d9-2795af91d8d9")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "RESET"
		(at -24.9028 -15.2752 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "dd226e45-cd07-42ec-88cb-c56cc8cac985")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.13)
			)
			(justify left top)
		)
	)
	(fp_text user "GND"
		(at -24.739 14.73958 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e07c5bf6-9395-439a-86b5-16ff87ac01fe")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A0"
		(at -14.2658 -15.77012 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e9eb0e2b-c579-4ae6-a18d-097833440bf1")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D40"
		(at 15.6691 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "eb2d9809-ce3e-441d-869d-8903b775aae6")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D44"
		(at 20.9242 -15.90062 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f1ae3f55-5b14-4784-8cdb-c326693d4883")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A13"
		(at 0.4418 -13.29562 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f7f19337-845b-48d8-bb6d-97a72c2a2a82")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "A10"
		(at -1.9887 -15.89712 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "fe20a729-d2d3-4930-ae3b-376d8e33df83")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(fp_text user "D8"
		(at -4.2152 14.85668 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ff538b3d-3f17-4aad-8f2f-8aedd915d3a4")
		(effects
			(font
				(size 0.52832 0.52832)
				(thickness 0.1057)
			)
			(justify left top)
		)
	)
	(pad "3V3@1" thru_hole oval
		(at -18.9 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0842e23a-2b91-4199-bd8e-5d1e2c6d6f89")
	)
	(pad "3V3@2" thru_hole oval
		(at -18.9 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "f60e7b53-7e09-4c70-a49d-6555a1bd4dfc")
	)
	(pad "5V@1" thru_hole oval
		(at -21.44 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "9e653168-285e-4caa-aee8-561680b7ce79")
	)
	(pad "5V@2" thru_hole oval
		(at -21.44 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "402512e3-8242-43bb-94b5-41b315515b6f")
	)
	(pad "5V@3" thru_hole oval
		(at 24.28 1.27)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "addd872e-830a-4aaa-b61b-8949a6297c42")
	)
	(pad "A0" thru_hole oval
		(at -13.82 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "7edcba46-95b9-4e89-907f-74e839a1ecd3")
	)
	(pad "A1" thru_hole oval
		(at -13.82 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "7515b4ce-2296-4112-86ea-b03c1c391768")
	)
	(pad "A2" thru_hole oval
		(at -11.28 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "b1715a3f-c911-4550-816f-6888a49aa591")
	)
	(pad "A3" thru_hole oval
		(at -11.28 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "76b2b098-ae50-4749-bcb8-39635ba9cd4c")
	)
	(pad "A4" thru_hole oval
		(at -8.74 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "9a4fec24-eb53-42d7-9337-fee092c7e3a5")
	)
	(pad "A5" thru_hole oval
		(at -8.74 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "85a0055c-711f-4e93-987e-a99b50b9c361")
	)
	(pad "A6" thru_hole oval
		(at -6.2 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "04ae0b2c-433d-4c6f-8326-3d22e368fdcf")
	)
	(pad "A7" thru_hole oval
		(at -6.2 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "f7c9fd89-334b-4bbc-8a29-9031dd4f3814")
	)
	(pad "A8" thru_hole oval
		(at -3.66 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "9e572aa2-6cf4-49fa-9202-0831a930a5f3")
	)
	(pad "A9" thru_hole oval
		(at -3.66 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "e8be9e5f-80cc-497a-b366-1788b1384d39")
	)
	(pad "A10" thru_hole oval
		(at -1.12 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "069f34ce-df49-4905-a939-be3b1a83ac1d")
	)
	(pad "A11" thru_hole oval
		(at -1.12 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "28427cd1-cc4d-4d76-a3d5-0691f479674c")
	)
	(pad "A12" thru_hole oval
		(at 1.42 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "e88cdc75-c6c7-443b-b9ac-3a45795a1aa7")
	)
	(pad "A13" thru_hole oval
		(at 1.42 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "b99d623b-9f0a-4a02-bacb-1a220745aae0")
	)
	(pad "A14" thru_hole oval
		(at 3.96 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0a07161e-b075-430b-8c3d-d7c6aabb1a61")
	)
	(pad "A15" thru_hole oval
		(at 3.96 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0cb1361b-05e0-432e-a3a4-19f1e7d987a7")
	)
	(pad "AREF" thru_hole oval
		(at -16.36 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "06c7399a-5fb6-442c-8dd4-6ea8c0af6ff1")
	)
	(pad "D2" thru_hole oval
		(at -11.28 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "572adb9a-66d2-4a37-b528-ff27235a432f")
	)
	(pad "D3" thru_hole oval
		(at -11.28 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "42efde9b-eff0-4d18-ba0d-c54d534031cb")
	)
	(pad "D4" thru_hole oval
		(at -8.74 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "449939b5-42de-4063-b43d-a81dcb702224")
	)
	(pad "D5" thru_hole oval
		(at -8.74 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "4ceec873-7e32-47fc-ad5a-8419f2fc5d3e")
	)
	(pad "D6" thru_hole oval
		(at -6.2 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "dd5ff74c-06e7-4408-8747-55104f8d68cd")
	)
	(pad "D7" thru_hole oval
		(at -6.2 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "de582834-85e3-4715-aee5-050c92f6cd52")
	)
	(pad "D8" thru_hole oval
		(at -3.66 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "99023fdb-51c1-4e5b-a679-e3234e5329bc")
	)
	(pad "D9" thru_hole oval
		(at -3.66 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "339da5c3-2b15-4c89-89af-7a9e94865fa3")
	)
	(pad "D10" thru_hole oval
		(at -1.12 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "26ca5901-093a-4cbf-8cd1-bd31c92c1469")
	)
	(pad "D11" thru_hole oval
		(at -1.12 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "36c7a3e5-a78c-402b-9720-27843b9b8716")
	)
	(pad "D12" thru_hole oval
		(at 1.42 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "84deff6a-8292-4620-9fa5-3e169245d9bc")
	)
	(pad "D13" thru_hole oval
		(at 1.42 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "aa289790-77c1-4fd0-b634-d6e78437fd04")
	)
	(pad "D14" thru_hole oval
		(at 3.96 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "33649d11-d600-4a92-8c84-0a274aa96634")
	)
	(pad "D15" thru_hole oval
		(at 3.96 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "fc68dbbf-df23-4ba6-8311-d03ae7766ddf")
	)
	(pad "D16" thru_hole oval
		(at 6.5 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "716c817e-61b9-433f-8432-fc9a94070bf6")
	)
	(pad "D17" thru_hole oval
		(at 6.5 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "5afc6e29-57cb-4427-be6e-f5eb95f94fcb")
	)
	(pad "D18" thru_hole oval
		(at 9.04 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "2161aeb8-94cb-4614-a5aa-5c495e2244a8")
	)
	(pad "D19" thru_hole oval
		(at 9.04 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "a56fdc41-f5db-4341-aa37-605fa23b59b7")
	)
	(pad "D20" thru_hole oval
		(at 11.58 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0df95703-7f65-4d41-aaf9-218588ca35cf")
	)
	(pad "D21" thru_hole oval
		(at 11.58 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "33e0790b-b643-474b-a54d-c626f0241087")
	)
	(pad "D22" thru_hole oval
		(at 14.12 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "51a1f1c7-5df5-4b70-b069-1c2434d39c16")
	)
	(pad "D23" thru_hole oval
		(at 14.12 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0fca367a-5ac8-4682-a2c5-6f11e0210937")
	)
	(pad "D24" thru_hole oval
		(at 16.66 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "25753953-c704-407e-8c5b-31629827639f")
	)
	(pad "D25" thru_hole oval
		(at 16.66 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "df8ea13b-2817-4f47-a870-6860f67ccba5")
	)
	(pad "D26" thru_hole oval
		(at 19.2 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0fbff1cc-25b6-4fcc-b776-53fd589befb2")
	)
	(pad "D27" thru_hole oval
		(at 19.2 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "6ae8e927-23b0-4b6b-8103-6ec3baffc2f3")
	)
	(pad "D28" thru_hole oval
		(at 21.74 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "5d4c965f-fdcf-4694-9887-e25e7db0cbb8")
	)
	(pad "D29" thru_hole oval
		(at 21.74 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "6d6311f5-4d55-48e3-86c8-0532de285d0d")
	)
	(pad "D30" thru_hole oval
		(at 24.28 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "0e3a1936-31c5-4aaf-85e7-08c20c3cc395")
	)
	(pad "D31" thru_hole oval
		(at 24.28 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "89cccda9-1eab-4939-816e-6c7787f2de50")
	)
	(pad "D32" thru_hole oval
		(at 6.5 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "dd5c1adf-884a-436d-a537-e893ec1cca01")
	)
	(pad "D33" thru_hole oval
		(at 6.5 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "b6f6a11b-c5c8-4c68-9236-813fa229788b")
	)
	(pad "D34" thru_hole oval
		(at 9.04 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "7daabf15-1eb4-4d41-b0c9-9b4e6c89cd7b")
	)
	(pad "D35" thru_hole oval
		(at 9.04 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "b1910c94-d58f-4f8d-9d77-e349e664e805")
	)
	(pad "D36" thru_hole oval
		(at 11.58 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "bcaf70a8-fbdf-4045-938c-5f91617d3bd9")
	)
	(pad "D37" thru_hole oval
		(at 11.58 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "978ee804-2615-43fb-858c-7bd24ad392b9")
	)
	(pad "D38" thru_hole oval
		(at 14.12 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "7f222688-acf6-43fc-accb-51d8e660cc6b")
	)
	(pad "D39" thru_hole oval
		(at 14.12 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "8fc39b8c-8887-467b-882b-549087b977da")
	)
	(pad "D40" thru_hole oval
		(at 16.66 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "f6002c67-f925-4c1d-9fc9-67f087635ead")
	)
	(pad "D41" thru_hole oval
		(at 16.66 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "efa8c144-9b44-4a50-be92-696de1314664")
	)
	(pad "D42" thru_hole oval
		(at 19.2 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "634a9144-6c17-462d-a6a8-2e4e24827bf4")
	)
	(pad "D43" thru_hole oval
		(at 19.2 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "4460b596-8b5c-4b4e-8de1-86a6a57f3857")
	)
	(pad "D44" thru_hole oval
		(at 21.74 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "fd6df7f7-832a-456b-95bd-e8d78fbc195c")
	)
	(pad "D45" thru_hole oval
		(at 21.74 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "bb5dc531-5f4c-4521-a252-64373c55c506")
	)
	(pad "D46" thru_hole oval
		(at 24.28 -16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "31187328-9da3-448a-a9ed-64160c3b0647")
	)
	(pad "D47" thru_hole oval
		(at 24.28 -13.97)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "ae2084eb-a25a-43e7-b938-ae0b78871bf6")
	)
	(pad "D48" thru_hole oval
		(at 24.28 -11.43)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "4f9d3962-86b4-4465-993b-5ff655691181")
	)
	(pad "D49" thru_hole oval
		(at 21.74 -11.43)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "1a9133c0-3288-432b-86bf-02f919d8d33e")
	)
	(pad "D50" thru_hole oval
		(at 24.28 -8.89)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "4db89c90-a746-46af-ab1d-6dff032d8a8a")
	)
	(pad "D51" thru_hole oval
		(at 21.74 -8.89)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "c6e2dc68-4282-4c12-bb97-fd4f96427948")
	)
	(pad "D52" thru_hole oval
		(at 24.28 -6.35)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "a016f001-104f-468c-a5ff-1395a8def4d6")
	)
	(pad "D53" thru_hole oval
		(at 21.74 -6.35)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "da99db01-357c-4c18-8f3b-913b6e15eb48")
	)
	(pad "GND@1" thru_hole oval
		(at -23.98 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "926d8318-4ef5-4d8f-a7c6-530705fdbde1")
	)
	(pad "GND@2" thru_hole oval
		(at -23.98 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "283c477e-2563-4628-ade3-5c6c4380b9a8")
	)
	(pad "GND@3" thru_hole oval
		(at 24.28 6.35)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "dfa4863a-adbd-4fbf-b1bf-c79c294f9c0c")
	)
	(pad "MISO" thru_hole oval
		(at 21.74 1.27)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "3229d2fd-e4ea-450c-a9a3-2172b938c77c")
	)
	(pad "MOSI" thru_hole oval
		(at 24.28 3.81)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "bad109fa-c503-4a42-b999-753462e65f8e")
	)
	(pad "RESET" thru_hole oval
		(at 21.74 6.35)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "2e138ff3-ef18-4809-ab9b-74823e793b1a")
	)
	(pad "RST" thru_hole oval
		(at -16.36 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "a021e1f5-dfda-467c-a501-d29e009720c0")
	)
	(pad "RX" thru_hole oval
		(at -13.82 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "e54df937-d2c3-4b75-b7a6-ef941f2eaed4")
	)
	(pad "SCK" thru_hole oval
		(at 21.74 3.81)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "32eef70d-db9e-445f-bdd9-25eda13ddf8c")
	)
	(pad "TX" thru_hole oval
		(at -13.82 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "3cb821ef-f5ff-43f3-b6b3-a0ab7f5cbd44")
	)
	(pad "VIN@1" thru_hole oval
		(at -26.52 19.05)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "75e21fb1-b92d-49d7-8a6f-5d63fe026534")
	)
	(pad "VIN@2" thru_hole oval
		(at -26.52 16.51)
		(size 2 2)
		(drill oval 1 0.9998)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "ad5ef45c-7788-4151-b85e-7604f392726a")
	)
	(embedded_fonts no)
)
